(kicad_symbol_lib (version 20220914) (generator qeda)
  (symbol "R0603" (pin_numbers hide) (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "R" (at 0.000 1.778 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "R0603" (at 0.000 -1.778 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "qeda:UC1608X55N" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "resistor, chip, 1.6x0.8 mm" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "R0603_1_1"
      (rectangle (start -2.540 1.016) (end 2.540 -1.016)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (pin passive line (at -3.810 0.000 0) (length 1.270)
        (name "L" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 3.810 0.000 180) (length 1.270)
        (name "R" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "C0603" (pin_numbers hide) (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "C" (at 0.000 2.794 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "C0603" (at 0.000 -2.794 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "qeda:CAPC1608X92N" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Chip capacitor 1.6x0.8 mm" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Capacitor" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "C0603_1_1"
      (polyline
        (pts
          (xy -0.381 2.032)
          (xy -0.381 -2.032)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.381 2.032)
          (xy 0.381 -2.032)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (pin passive line (at -2.540 0.000 0) (length 2.159)
        (name "L" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.540 0.000 180) (length 2.159)
        (name "R" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "LED0805" (pin_numbers hide) (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "D" (at 0.000 2.032 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "LED0805" (at 0.000 -2.032 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "qeda:UPC2012X80N" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "diode, LED, chip, 2.0x1.2 mm" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LED0805_1_1"
      (polyline
        (pts (xy -1.016 1.270) (xy 1.016 0.000) (xy -1.016 -1.270) (xy -1.016 1.270))
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 1.016 1.270)
          (xy 1.016 -1.270)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.270 1.905)
          (xy 2.540 3.175)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts (xy 1.725 2.720) (xy 2.540 3.175) (xy 2.085 2.360) (xy 1.725 2.720))
        (stroke (width 0.305) (type default))
        (fill (type outline))
      )
      (polyline
        (pts
          (xy 1.905 1.270)
          (xy 3.175 2.540)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts (xy 2.360 2.085) (xy 3.175 2.540) (xy 2.720 1.725) (xy 2.360 2.085))
        (stroke (width 0.305) (type default))
        (fill (type outline))
      )
      (pin passive line (at -2.540 0.000 0) (length 1.524)
        (name "A" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.540 0.000 180) (length 1.524)
        (name "C" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "XLR-15-N3L" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 11.430 0.762 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "XLR-15-N3L" (at 12.192 -18.542 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "qeda:CONNECTOR_XLR-15-N3L" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheet.lcsc.com/lcsc/2005251832_JINJIA-XLR-15-N3L_C558606.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "XLR connector, 3-pin, male" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "XLR-15-N3L_1_1"
      (rectangle (start 0.000 0.000) (end 22.860 -17.780)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (pin passive line (at 27.940 -2.540 180) (length 5.080)
        (name "PINS" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 27.940 -5.080 180) (length 5.080)
        (name "PINS" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 27.940 -7.620 180) (length 5.080)
        (name "PINS" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 11.430 -22.860 90) (length 5.080)
        (name "SHIELD" (effects (font (size 1.27 1.27))))
        (number "G" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "XLR-18P-2-N3B" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 5.715 0.762 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "XLR-18P-2-N3B" (at 5.715 -10.922 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "qeda:CONNECTOR_XLR-18P-2-N3B" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheet.lcsc.com/lcsc/2005251832_JINJIA-XLR-18P-2-N3B_C558734.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "XLR connector, 3-pin, female" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "XLR-18P-2-N3B_1_1"
      (rectangle (start 0.000 0.000) (end 11.430 -10.160)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (pin passive line (at 16.510 -2.540 180) (length 5.080)
        (name "PINS" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 16.510 -5.080 180) (length 5.080)
        (name "PINS" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 16.510 -7.620 180) (length 5.080)
        (name "PINS" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "HC-RJ45-5JA-1-5" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 11.430 0.762 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "HC-RJ45-5JA-1-5" (at 11.430 -23.622 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "qeda:CONNECTOR_HC-RJ45-5JA-1-5" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheet.lcsc.com/lcsc/2204251600_HCTL-HC-RJ45-5JA-1-5-Y_C3000187.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "connector, RJ45, with LEDs" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "HC-RJ45-5JA-1-5_1_1"
      (rectangle (start 0.000 0.000) (end 22.860 -22.860)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (pin passive line (at -5.080 -6.350 0) (length 5.080)
        (name "LEDA_L" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.080 -8.890 0) (length 5.080)
        (name "LEDC_L" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.080 -13.970 0) (length 5.080)
        (name "LEDA_R" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.080 -16.510 0) (length 5.080)
        (name "LEDC_R" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 27.940 -2.540 180) (length 5.080)
        (name "8P8C" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 27.940 -5.080 180) (length 5.080)
        (name "8P8C" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 27.940 -7.620 180) (length 5.080)
        (name "8P8C" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 27.940 -10.160 180) (length 5.080)
        (name "8P8C" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 27.940 -12.700 180) (length 5.080)
        (name "8P8C" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 27.940 -15.240 180) (length 5.080)
        (name "8P8C" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 27.940 -17.780 180) (length 5.080)
        (name "8P8C" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 27.940 -20.320 180) (length 5.080)
        (name "8P8C" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "JK60-110" (pin_numbers hide) (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "F" (at 0.000 1.778 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "JK60-110" (at 0.000 -1.778 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "qeda:VREG_JK60-110" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheet.lcsc.com/lcsc/2304140030_Jinrui-Electronic-Materials-Co--JK60-110_C369088.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "PPTC resettable fuse" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "JK60-110_1_1"
      (rectangle (start -2.540 1.016) (end 2.540 -1.016)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -2.540 0.000)
          (xy 2.540 0.000)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (pin passive line (at -3.810 0.000 0) (length 1.270)
        (name "L" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 3.810 0.000 180) (length 1.270)
        (name "R" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "DC-005_2.0" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 6.985 0.762 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "DC-005_2.0" (at 6.985 -16.002 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "qeda:CONNECTOR_DC-005_2.0" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheet.lcsc.com/lcsc/1811051112_BOOMELE-Boom-Precision-Elec-DC-005-2-0_C16214.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "barrel DC power jack" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "connector, barrel" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "DC-005_2.0_1_1"
      (rectangle (start 0.000 0.000) (end 13.970 -15.240)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (pin passive line (at 19.050 -2.540 180) (length 5.080)
        (name "PIN" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 19.050 -7.620 180) (length 5.080)
        (name "SWITCH" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 19.050 -12.700 180) (length 5.080)
        (name "COM" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MX25C-7.62-02P" (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 2.540 0.762 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "MX25C-7.62-02P" (at 2.540 -8.382 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "qeda:CONNECTOR_MX25C-7.62-02P" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.lcsc.com/product-detail/Barrier-Terminal-Blocks_MAX-MX25C-7-62-02P-BK01-Cu-S-A_C5188509.html" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "barrier terminal, 7.62mm pitch" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MX25C-7.62-02P_1_1"
      (rectangle (start 0.000 0.000) (end 5.080 -7.620)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (pin passive line (at -5.080 -2.540 0) (length 5.080)
        (name "1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.080 -5.080 0) (length 5.080)
        (name "2" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "KF250-3.5-08P-1" (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 2.540 0.762 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "KF250-3.5-08P-1" (at 2.540 -23.622 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "qeda:CONNECTOR_KF250-3.5-08P-1" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://a3.ldycdn.com/KF250-3.5-aidqkBpqKirRljSkrnijolli.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "spring loaded terminal, with lever, 3.5 mm pitch, vertical insertion" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "KF250-3.5-08P-1_1_1"
      (rectangle (start 0.000 0.000) (end 5.080 -22.860)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (pin passive line (at -5.080 -2.540 0) (length 5.080)
        (name "1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.080 -5.080 0) (length 5.080)
        (name "2" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.080 -7.620 0) (length 5.080)
        (name "3" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.080 -10.160 0) (length 5.080)
        (name "4" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.080 -12.700 0) (length 5.080)
        (name "5" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.080 -15.240 0) (length 5.080)
        (name "6" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.080 -17.780 0) (length 5.080)
        (name "7" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.080 -20.320 0) (length 5.080)
        (name "8" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "SCHOTTKY" (pin_numbers hide) (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "D" (at 0.000 2.032 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "SCHOTTKY" (at 0.000 -2.032 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "qeda:UPM4326X290N" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "diode, schottky, generic" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SCHOTTKY_1_1"
      (polyline
        (pts (xy -1.016 1.270) (xy 1.016 0.000) (xy -1.016 -1.270) (xy -1.016 1.270))
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 1.016 1.270)
          (xy 1.016 -1.270)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.016 -1.270)
          (xy 0.508 -1.270)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.508 -1.270)
          (xy 0.508 -0.762)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.016 1.270)
          (xy 1.524 1.270)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.524 1.270)
          (xy 1.524 0.762)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (pin passive line (at -2.540 0.000 0) (length 1.524)
        (name "A" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.540 0.000 180) (length 1.524)
        (name "C" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "TX4137" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 6.350 0.762 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "TX4137" (at 7.112 -12.192 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "qeda:SOT95P280X80-6N" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "step-down buck converter" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TX4137_1_1"
      (rectangle (start 0.000 0.000) (end 12.700 -11.430)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (pin power_in line (at -5.080 -2.540 0) (length 5.080)
        (name "IN" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.080 -7.620 0) (length 5.080)
        (name "EN" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 17.780 -2.540 180) (length 5.080)
        (name "SW" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 17.780 -7.620 180) (length 5.080)
        (name "FB" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 6.350 -16.510 90) (length 5.080)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "XC6206" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 8.255 0.762 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "XC6206" (at 8.382 -9.652 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "qeda:SOT95P280X130-3N" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.torexsemi.com/file/xc6206/XC6206.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "positive voltage regulators" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "IC, regulator" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "XC6206_1_1"
      (rectangle (start 0.000 0.000) (end 16.510 -8.890)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (pin power_in line (at -5.080 -2.540 0) (length 5.080)
        (name "VIN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at 21.590 -2.540 180) (length 5.080)
        (name "VOUT" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 7.620 -13.970 90) (length 5.080)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "L4540" (pin_numbers hide) (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "L" (at 0.000 2.032 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "L4540" (at 0.000 -0.762 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "qeda:INDUCTOR_L4540" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "power inductor, SMD, 4.5x4.0mm" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "inductor" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "L4540_1_1"
      (arc (start -5.080 0.000) (mid -3.810 1.270) (end -2.540 0.000)
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (arc (start -2.540 0.000) (mid -1.270 1.270) (end 0.000 0.000)
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (arc (start 0.000 0.000) (mid 1.270 1.270) (end 2.540 0.000)
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (arc (start 2.540 0.000) (mid 3.810 1.270) (end 5.080 0.000)
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (pin passive line (at -6.350 0.000 0) (length 1.270)
        (name "L" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 6.350 0.000 180) (length 1.270)
        (name "R" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "CH32V203CxT" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0.000 0.762 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "CH32V203CxT" (at 21.082 -56.642 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "qeda:QFP50P900X900X150-48N" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.wch-ic.com/downloads/CH32V203DS0_PDF.html" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "RISC-V micro-controller" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "MCU, Micro-Controller" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "CH32V203CxT_1_1"
      (rectangle (start 0.000 0.000) (end 41.910 -55.880)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (pin input line (at -5.080 -2.540 0) (length 5.080)
        (name "BOOT0" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.080 -5.080 0) (length 5.080)
        (name "OSC_IN" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.080 -7.620 0) (length 5.080)
        (name "OSC_OUT" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -5.080 -10.160 0) (length 5.080)
        (name "NRST" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -15.240 0) (length 5.080)
        (name "PA0-WKUP" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -17.780 0) (length 5.080)
        (name "PA1" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -20.320 0) (length 5.080)
        (name "PA2" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -22.860 0) (length 5.080)
        (name "PA3" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -25.400 0) (length 5.080)
        (name "PA4" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -27.940 0) (length 5.080)
        (name "PA5" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -30.480 0) (length 5.080)
        (name "PA6" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -33.020 0) (length 5.080)
        (name "PA7" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -35.560 0) (length 5.080)
        (name "PA8" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -38.100 0) (length 5.080)
        (name "PA9" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -40.640 0) (length 5.080)
        (name "PA10" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -43.180 0) (length 5.080)
        (name "PA11" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -45.720 0) (length 5.080)
        (name "PA12" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -48.260 0) (length 5.080)
        (name "PA13" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -50.800 0) (length 5.080)
        (name "PA14" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -53.340 0) (length 5.080)
        (name "PA15" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 46.990 -3.810 180) (length 5.080)
        (name "PB0" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 46.990 -6.350 180) (length 5.080)
        (name "PB1" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 46.990 -8.890 180) (length 5.080)
        (name "PB2" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 46.990 -11.430 180) (length 5.080)
        (name "PB3" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 46.990 -13.970 180) (length 5.080)
        (name "PB4" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 46.990 -16.510 180) (length 5.080)
        (name "PB5" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 46.990 -19.050 180) (length 5.080)
        (name "PB6" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 46.990 -21.590 180) (length 5.080)
        (name "PB7" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 46.990 -24.130 180) (length 5.080)
        (name "PB8" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 46.990 -26.670 180) (length 5.080)
        (name "PB9" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 46.990 -29.210 180) (length 5.080)
        (name "PB10" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 46.990 -31.750 180) (length 5.080)
        (name "PB11" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 46.990 -34.290 180) (length 5.080)
        (name "PB12" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 46.990 -36.830 180) (length 5.080)
        (name "PB13" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 46.990 -39.370 180) (length 5.080)
        (name "PB14" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 46.990 -41.910 180) (length 5.080)
        (name "PB15" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 46.990 -46.990 180) (length 5.080)
        (name "PC13-TAMPER-RTC" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 46.990 -49.530 180) (length 5.080)
        (name "PC14-OSC32_IN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 46.990 -52.070 180) (length 5.080)
        (name "PC15-OSC32_OUT" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 11.430 5.080 270) (length 5.080)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 13.970 5.080 270) (length 5.080)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 16.510 5.080 270) (length 5.080)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 19.050 5.080 270) (length 5.080)
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 21.590 5.080 270) (length 5.080)
        (name "VBAT" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 12.700 -60.960 90) (length 5.080)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 15.240 -60.960 90) (length 5.080)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.780 -60.960 90) (length 5.080)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 20.320 -60.960 90) (length 5.080)
        (name "VSSA" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MOV_1206" (pin_numbers hide) (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "R" (at 0.000 1.778 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "MOV_1206" (at 0.000 -1.778 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "qeda:VARC3216X190N" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "metal-oxide varistor" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "varistor" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MOV_1206_1_1"
      (rectangle (start -2.540 1.016) (end 2.540 -1.016)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (pin passive line (at -3.810 0.000 0) (length 1.270)
        (name "L" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 3.810 0.000 180) (length 1.270)
        (name "R" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MAX3485ESA" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0.000 0.762 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "MAX3485ESA" (at 7.112 -21.082 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "qeda:SOP127P600X175-8N" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.analog.com/en/products/max3485.html" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "transceiver, RS-485/RS-422, 3.3V powered" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MAX3485ESA_1_1"
      (rectangle (start 0.000 0.000) (end 10.160 -20.320)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (pin output line (at -5.080 -2.540 0) (length 5.080)
        (name "RO" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -5.080 -7.620 0) (length 5.080)
        (name "~{RE}" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.080 -12.700 0) (length 5.080)
        (name "DE" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.080 -17.780 0) (length 5.080)
        (name "DI" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.240 -7.620 180) (length 5.080)
        (name "A" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.240 -12.700 180) (length 5.080)
        (name "B" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 6.350 5.080 270) (length 5.080)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 6.350 -25.400 90) (length 5.080)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ADM2483" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0.000 0.762 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "ADM2483" (at 16.002 -18.542 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "qeda:SOIC127P1030X265-16N" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADM2483.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "transceiver, RS-485, isolated" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ADM2483_1_1"
      (rectangle (start 0.000 0.000) (end 20.320 -17.780)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (pin input line (at -5.080 -2.540 0) (length 5.080)
        (name "DE" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.080 -5.080 0) (length 5.080)
        (name "TxD" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -5.080 -7.620 0) (length 5.080)
        (name "RxD" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input inverted (at -5.080 -10.160 0) (length 5.080)
        (name "~{RE}" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.080 -15.240 0) (length 5.080)
        (name "PV" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.400 -7.620 180) (length 5.080)
        (name "A" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.400 -10.160 180) (length 5.080)
        (name "B" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.160 5.080 270) (length 5.080)
        (name "VDD1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 12.700 5.080 270) (length 5.080)
        (name "VDD2" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 7.620 -22.860 90) (length 5.080)
        (name "GND1" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.160 -22.860 90) (length 5.080)
        (name "GND1" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 12.700 -22.860 90) (length 5.080)
        (name "GND2" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 15.240 -22.860 90) (length 5.080)
        (name "GND2" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "BxxxxS" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 5.715 0.762 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "BxxxxS" (at 5.715 -10.922 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "qeda:VREG_BXXXXS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.mornsun-power.com/public/uploads/pdf/B05_S-1WR3.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "DC/DC converter, isolated" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "BxxxxS_1_1"
      (rectangle (start 0.000 0.000) (end 11.430 -10.160)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (pin power_in line (at -5.080 -2.540 0) (length 5.080)
        (name "VIN" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -5.080 -7.620 0) (length 5.080)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 16.510 -2.540 180) (length 5.080)
        (name "VO" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 16.510 -7.620 180) (length 5.080)
        (name "0V" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "C1206" (pin_numbers hide) (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "C" (at 0.000 2.794 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "C1206" (at 0.000 -2.794 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "qeda:CAPC3216X180N" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Chip capacitor 3.2x1.6 mm" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Capacitor" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "C1206_1_1"
      (polyline
        (pts
          (xy -0.381 2.032)
          (xy -0.381 -2.032)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.381 2.032)
          (xy 0.381 -2.032)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (pin passive line (at -2.540 0.000 0) (length 2.159)
        (name "L" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.540 0.000 180) (length 2.159)
        (name "R" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "ZENER_SOD523" (pin_numbers hide) (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "D" (at 0.000 2.540 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "ZENER_SOD523" (at 0.000 -2.540 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "qeda:SODFL1608X65N" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "diode, zener" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Diode, Zener" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "ZENER_SOD523_1_1"
      (polyline
        (pts (xy -1.016 1.270) (xy 1.016 0.000) (xy -1.016 -1.270) (xy -1.016 1.270))
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 1.016 1.270)
          (xy 1.016 -1.270)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.016 1.270)
          (xy 0.508 1.778)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.016 -1.270)
          (xy 1.524 -1.778)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (pin passive line (at -2.540 0.000 0) (length 1.524)
        (name "A" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.540 0.000 180) (length 1.524)
        (name "C" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "LED0603" (pin_numbers hide) (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "D" (at 0.000 2.032 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "LED0603" (at 0.000 -2.032 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "qeda:UPC1608X90N" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "diode, LED, chip, 1.6x0.8 mm" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LED0603_1_1"
      (polyline
        (pts (xy -1.016 1.270) (xy 1.016 0.000) (xy -1.016 -1.270) (xy -1.016 1.270))
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 1.016 1.270)
          (xy 1.016 -1.270)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.270 1.905)
          (xy 2.540 3.175)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts (xy 1.725 2.720) (xy 2.540 3.175) (xy 2.085 2.360) (xy 1.725 2.720))
        (stroke (width 0.305) (type default))
        (fill (type outline))
      )
      (polyline
        (pts
          (xy 1.905 1.270)
          (xy 3.175 2.540)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts (xy 2.360 2.085) (xy 3.175 2.540) (xy 2.720 1.725) (xy 2.360 2.085))
        (stroke (width 0.305) (type default))
        (fill (type outline))
      )
      (pin passive line (at -2.540 0.000 0) (length 1.524)
        (name "A" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.540 0.000 180) (length 1.524)
        (name "C" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "HC-49_SM" (pin_numbers hide) (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "Y" (at 0.000 2.794 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "HC-49_SM" (at 0.000 -2.794 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "qeda:XTAL114X47X400N" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.farnell.com/datasheets/321153.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "crystal oscillator in HC-49 case" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "oscillator, crystal" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "HC-49_SM_1_1"
      (rectangle (start -0.762 2.032) (end 0.762 -2.032)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -1.524 1.016)
          (xy -1.524 -1.016)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.524 1.016)
          (xy 1.524 -1.016)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (pin passive line (at -3.810 0.000 0) (length 2.286)
        (name "L" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 3.810 0.000 180) (length 2.286)
        (name "R" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "HEADER-2.54-2x3" (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 3.810 0.762 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "HEADER-2.54-2x3" (at 3.810 -10.922 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "qeda:CONNECTOR_HEADER-2.54-2X3" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/54101.pdf https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/67996.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "header, 1 rows, 0.1 in/2.54 mm pitch, through hole, straight, not shrouded" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Connector, Male" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "HEADER-2.54-2x3_1_1"
      (rectangle (start 0.000 0.000) (end 7.620 -10.160)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (pin passive line (at -5.080 -2.540 0) (length 5.080)
        (name "1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.080 -5.080 0) (length 5.080)
        (name "3" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.080 -7.620 0) (length 5.080)
        (name "5" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.700 -2.540 180) (length 5.080)
        (name "2" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.700 -5.080 180) (length 5.080)
        (name "4" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 12.700 -7.620 180) (length 5.080)
        (name "6" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "1TS002E" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 6.350 0.762 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "1TS002E" (at 6.350 -5.842 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "qeda:MECHANICAL_1TS002E" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheet.lcsc.com/lcsc/1811071030_HYP-Hongyuan-Precision-1TS002E-2700-2500-CT_C319367.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "SPST tactical momentary switch, SMD 6.1x3.7x2.5mm" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "1TS002E_1_1"
      (rectangle (start 0.000 0.000) (end 12.700 -5.080)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (pin passive line (at -5.080 -2.540 0) (length 5.080)
        (name "1" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 17.780 -2.540 180) (length 5.080)
        (name "2" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "TS-1187A" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 6.350 0.762 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "TS-1187A" (at 6.350 -8.382 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "qeda:MECHANICAL_TS-1187A" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.helloxkb.com/public/images/pdf/TS-1187A-X-X-X.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "dual tactical momentary switch, SMD 5.1*5.1*1.5mm" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TS-1187A_1_1"
      (rectangle (start 0.000 0.000) (end 12.700 -7.620)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (pin passive line (at -5.080 -2.540 0) (length 5.080)
        (name "A" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.080 -5.080 0) (length 5.080)
        (name "B" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 17.780 -2.540 180) (length 5.080)
        (name "C" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 17.780 -5.080 180) (length 5.080)
        (name "D" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
