(kicad_symbol_lib (version 20220914) (generator qeda)
  (symbol "R0603" (pin_numbers hide) (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "R" (at 0.000 1.778 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "R0603" (at 0.000 -1.778 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "qeda:UC1608X55N" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "resistor, chip, 1.6x0.8 mm" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "R0603_1_1"
      (rectangle (start -2.540 1.016) (end 2.540 -1.016)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (pin passive line (at -3.810 0.000 0) (length 1.270)
        (name "L" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 3.810 0.000 180) (length 1.270)
        (name "R" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "C0603" (pin_numbers hide) (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "C" (at 0.000 2.794 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "C0603" (at 0.000 -2.794 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "qeda:CAPC1608X92N" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "Chip capacitor 1.6x0.8 mm" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Capacitor" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "C0603_1_1"
      (polyline
        (pts
          (xy -0.381 2.032)
          (xy -0.381 -2.032)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.381 2.032)
          (xy 0.381 -2.032)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (pin passive line (at -2.540 0.000 0) (length 2.159)
        (name "L" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.540 0.000 180) (length 2.159)
        (name "R" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "LED0805" (pin_numbers hide) (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "D" (at 0.000 2.032 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "LED0805" (at 0.000 -2.032 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "qeda:UPC2012X80N" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "diode, LED, chip, 2.0x1.2 mm" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LED0805_1_1"
      (polyline
        (pts (xy -1.016 1.270) (xy 1.016 0.000) (xy -1.016 -1.270) (xy -1.016 1.270))
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 1.016 1.270)
          (xy 1.016 -1.270)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.270 1.905)
          (xy 2.540 3.175)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts (xy 1.725 2.720) (xy 2.540 3.175) (xy 2.085 2.360) (xy 1.725 2.720))
        (stroke (width 0.305) (type default))
        (fill (type outline))
      )
      (polyline
        (pts
          (xy 1.905 1.270)
          (xy 3.175 2.540)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts (xy 2.360 2.085) (xy 3.175 2.540) (xy 2.720 1.725) (xy 2.360 2.085))
        (stroke (width 0.305) (type default))
        (fill (type outline))
      )
      (pin passive line (at -2.540 0.000 0) (length 1.524)
        (name "A" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.540 0.000 180) (length 1.524)
        (name "C" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "XKB_U262-24XN-4BV60" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 0.000 0.762 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "XKB_U262-24XN-4BV60" (at 97.282 -54.102 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "qeda:CONNECTOR_XKB_U262-24XN-4BV60" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.helloxkb.com/public/images/pdf/U262-24XN-4BV60.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "connector, USB-C, receptacle, 24-pin, SMT+THT+TABS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "XKB_U262-24XN-4BV60_1_1"
      (rectangle (start 0.000 0.000) (end 43.180 -53.340)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (pin output line (at -5.080 -5.080 0) (length 5.080)
        (name "TX1+" (effects (font (size 1.27 1.27))))
        (number "A2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -5.080 -7.620 0) (length 5.080)
        (name "TX1-" (effects (font (size 1.27 1.27))))
        (number "A3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -10.160 0) (length 5.080)
        (name "CC1" (effects (font (size 1.27 1.27))))
        (number "A5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -12.700 0) (length 5.080)
        (name "D+" (effects (font (size 1.27 1.27))))
        (number "A6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -15.240 0) (length 5.080)
        (name "D-" (effects (font (size 1.27 1.27))))
        (number "A7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -17.780 0) (length 5.080)
        (name "SBU1" (effects (font (size 1.27 1.27))))
        (number "A8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.080 -20.320 0) (length 5.080)
        (name "RX2-" (effects (font (size 1.27 1.27))))
        (number "A10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.080 -22.860 0) (length 5.080)
        (name "RX2+" (effects (font (size 1.27 1.27))))
        (number "A11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 48.260 -5.080 180) (length 5.080)
        (name "RX1+" (effects (font (size 1.27 1.27))))
        (number "B11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 48.260 -7.620 180) (length 5.080)
        (name "RX1-" (effects (font (size 1.27 1.27))))
        (number "B10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 48.260 -10.160 180) (length 5.080)
        (name "SBU2" (effects (font (size 1.27 1.27))))
        (number "B8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 48.260 -12.700 180) (length 5.080)
        (name "D-" (effects (font (size 1.27 1.27))))
        (number "B7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 48.260 -15.240 180) (length 5.080)
        (name "D+" (effects (font (size 1.27 1.27))))
        (number "B6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 48.260 -17.780 180) (length 5.080)
        (name "CC2" (effects (font (size 1.27 1.27))))
        (number "B5" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 48.260 -20.320 180) (length 5.080)
        (name "TX2-" (effects (font (size 1.27 1.27))))
        (number "B3" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 48.260 -22.860 180) (length 5.080)
        (name "TX2+" (effects (font (size 1.27 1.27))))
        (number "B2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.780 5.080 270) (length 5.080)
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "A4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 20.320 5.080 270) (length 5.080)
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "A9" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.860 5.080 270) (length 5.080)
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "B4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 25.400 5.080 270) (length 5.080)
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "B9" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 11.430 -58.420 90) (length 5.080)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "A1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 13.970 -58.420 90) (length 5.080)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "A12" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 16.510 -58.420 90) (length 5.080)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "B1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 19.050 -58.420 90) (length 5.080)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "B12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 31.750 -58.420 90) (length 5.080)
        (name "SHIELD/SHIELD/SHIELD/SHIELD" (effects (font (size 1.27 1.27))))
        (number "S1" (effects (font (size 1.27 1.27))))
        (alternate "SHIELD" passive line)
        (alternate "SHIELD" passive line)
        (alternate "SHIELD" passive line)
      )
      (pin passive line (at 53.340 -58.420 90) (length 5.080)
        (name "SHIELD/SHIELD/SHIELD/SHIELD" (effects (font (size 1.27 1.27))))
        (number "S1" (effects (font (size 1.27 1.27))))
        (alternate "SHIELD" passive line)
        (alternate "SHIELD" passive line)
        (alternate "SHIELD" passive line)
      )
      (pin passive line (at 74.930 -58.420 90) (length 5.080)
        (name "SHIELD/SHIELD/SHIELD/SHIELD" (effects (font (size 1.27 1.27))))
        (number "S1" (effects (font (size 1.27 1.27))))
        (alternate "SHIELD" passive line)
        (alternate "SHIELD" passive line)
        (alternate "SHIELD" passive line)
      )
      (pin passive line (at 96.520 -58.420 90) (length 5.080)
        (name "SHIELD/SHIELD/SHIELD/SHIELD" (effects (font (size 1.27 1.27))))
        (number "S1" (effects (font (size 1.27 1.27))))
        (alternate "SHIELD" passive line)
        (alternate "SHIELD" passive line)
        (alternate "SHIELD" passive line)
      )
    )
  )
  (symbol "USB_2_MICRO-B_XKB_U254-051N" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 13.970 0.762 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "USB_2_MICRO-B_XKB_U254-051N" (at 60.452 -42.672 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "qeda:CONNECTOR_USB_2_MICRO-B_XKB_U254-051N" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheet.lcsc.com/lcsc/2107141638_XKB-Connectivity-U254-051N-4BH806_C319170.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "USB 2.0 micro receptacle, type B, SMT" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "connector, usb" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "USB_2_MICRO-B_XKB_U254-051N_1_1"
      (rectangle (start 0.000 0.000) (end 27.940 -41.910)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (pin power_in line (at 33.020 -2.540 180) (length 5.080)
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 33.020 -5.080 180) (length 5.080)
        (name "D-" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 33.020 -7.620 180) (length 5.080)
        (name "D+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 33.020 -10.160 180) (length 5.080)
        (name "ID" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 33.020 -12.700 180) (length 5.080)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 17.780 -46.990 90) (length 5.080)
        (name "SHELL/SHELL/SHELL/SHELL" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
        (alternate "SHELL" passive line)
        (alternate "SHELL" passive line)
        (alternate "SHELL" passive line)
      )
      (pin passive line (at 31.750 -46.990 90) (length 5.080)
        (name "SHELL/SHELL/SHELL/SHELL" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
        (alternate "SHELL" passive line)
        (alternate "SHELL" passive line)
        (alternate "SHELL" passive line)
      )
      (pin passive line (at 45.720 -46.990 90) (length 5.080)
        (name "SHELL/SHELL/SHELL/SHELL" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
        (alternate "SHELL" passive line)
        (alternate "SHELL" passive line)
        (alternate "SHELL" passive line)
      )
      (pin passive line (at 59.690 -46.990 90) (length 5.080)
        (name "SHELL/SHELL/SHELL/SHELL" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
        (alternate "SHELL" passive line)
        (alternate "SHELL" passive line)
        (alternate "SHELL" passive line)
      )
    )
  )
  (symbol "U231-09XN-4BLRA00" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 0.000 0.762 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "U231-09XN-4BLRA00" (at 45.212 -40.132 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "qeda:CONNECTOR_U231-09XN-4BLRA00" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "http://www.helloxkb.com/public/images/pdf/U231-091N-4BLRA00-S.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "connector, USB-A, receptacle, USB 3.0, SMT+TABS" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "U231-09XN-4BLRA00_1_1"
      (rectangle (start 0.000 0.000) (end 38.100 -39.370)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (pin bidirectional line (at 43.180 -5.080 180) (length 5.080)
        (name "D-" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 43.180 -10.160 180) (length 5.080)
        (name "D+" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 43.180 -15.240 180) (length 5.080)
        (name "SSRX-" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 43.180 -20.320 180) (length 5.080)
        (name "SSRX+" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 43.180 -25.400 180) (length 5.080)
        (name "SSTX-" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 43.180 -30.480 180) (length 5.080)
        (name "SSTX+" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 19.050 5.080 270) (length 5.080)
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 12.700 -44.450 90) (length 5.080)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.780 -44.450 90) (length 5.080)
        (name "GND_DRAIN" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 25.400 -44.450 90) (length 5.080)
        (name "SHIELD/SHIELD" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
        (alternate "SHIELD" passive line)
      )
      (pin passive line (at 44.450 -44.450 90) (length 5.080)
        (name "SHIELD/SHIELD" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
        (alternate "SHIELD" passive line)
      )
    )
  )
  (symbol "LED0603" (pin_numbers hide) (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "D" (at 0.000 2.032 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "LED0603" (at 0.000 -2.032 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "qeda:UPC1608X90N" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "diode, LED, chip, 1.6x0.8 mm" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "LED0603_1_1"
      (polyline
        (pts (xy -1.016 1.270) (xy 1.016 0.000) (xy -1.016 -1.270) (xy -1.016 1.270))
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 1.016 1.270)
          (xy 1.016 -1.270)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.270 1.905)
          (xy 2.540 3.175)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts (xy 1.725 2.720) (xy 2.540 3.175) (xy 2.085 2.360) (xy 1.725 2.720))
        (stroke (width 0.305) (type default))
        (fill (type outline))
      )
      (polyline
        (pts
          (xy 1.905 1.270)
          (xy 3.175 2.540)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts (xy 2.360 2.085) (xy 3.175 2.540) (xy 2.720 1.725) (xy 2.360 2.085))
        (stroke (width 0.305) (type default))
        (fill (type outline))
      )
      (pin passive line (at -2.540 0.000 0) (length 1.524)
        (name "A" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.540 0.000 180) (length 1.524)
        (name "C" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "HRO_TYPE-C-31-M-17" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 0.000 0.762 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "HRO_TYPE-C-31-M-17" (at 79.502 -50.292 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "qeda:CONNECTOR_HRO_TYPE-C-31-M-17" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheet.lcsc.com/lcsc/2108131830_Korean-Hroparts-Elec-TYPE-C-31-M-17_C283540.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "connector, USB-C, receptacle, 6-pin, SMD only" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "HRO_TYPE-C-31-M-17_1_1"
      (rectangle (start 0.000 0.000) (end 35.560 -49.530)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (pin bidirectional line (at -5.080 -10.160 0) (length 5.080)
        (name "CC1" (effects (font (size 1.27 1.27))))
        (number "A5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 40.640 -10.160 180) (length 5.080)
        (name "CC2" (effects (font (size 1.27 1.27))))
        (number "B5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 16.510 5.080 270) (length 5.080)
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "A9" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 19.050 5.080 270) (length 5.080)
        (name "VBUS" (effects (font (size 1.27 1.27))))
        (number "B9" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 10.160 -54.610 90) (length 5.080)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "A12" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 12.700 -54.610 90) (length 5.080)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "B12" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 25.400 -54.610 90) (length 5.080)
        (name "SHIELD/SHIELD/SHIELD/SHIELD" (effects (font (size 1.27 1.27))))
        (number "S1" (effects (font (size 1.27 1.27))))
        (alternate "SHIELD" passive line)
        (alternate "SHIELD" passive line)
        (alternate "SHIELD" passive line)
      )
      (pin passive line (at 43.180 -54.610 90) (length 5.080)
        (name "SHIELD/SHIELD/SHIELD/SHIELD" (effects (font (size 1.27 1.27))))
        (number "S1" (effects (font (size 1.27 1.27))))
        (alternate "SHIELD" passive line)
        (alternate "SHIELD" passive line)
        (alternate "SHIELD" passive line)
      )
      (pin passive line (at 60.960 -54.610 90) (length 5.080)
        (name "SHIELD/SHIELD/SHIELD/SHIELD" (effects (font (size 1.27 1.27))))
        (number "S1" (effects (font (size 1.27 1.27))))
        (alternate "SHIELD" passive line)
        (alternate "SHIELD" passive line)
        (alternate "SHIELD" passive line)
      )
      (pin passive line (at 78.740 -54.610 90) (length 5.080)
        (name "SHIELD/SHIELD/SHIELD/SHIELD" (effects (font (size 1.27 1.27))))
        (number "S1" (effects (font (size 1.27 1.27))))
        (alternate "SHIELD" passive line)
        (alternate "SHIELD" passive line)
        (alternate "SHIELD" passive line)
      )
    )
  )
  (symbol "MY-2032-12" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0.000 0.762 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "MY-2032-12" (at 7.112 -24.892 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "qeda:CONNECTOR_MY-2032-12" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://datasheet.lcsc.com/lcsc/2012181809_MYOUNG-MY-2032-12_C964833.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "coin cell battery holder, CR2032, SMD, folded metal" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MY-2032-12_1_1"
      (rectangle (start 0.000 0.000) (end 10.160 -24.130)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (pin power_in line (at 7.620 5.080 270) (length 5.080)
        (name "BAT+L/BAT+R" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
        (alternate "BAT+R" power_in line)
      )
      (pin power_in line (at 13.970 5.080 270) (length 5.080)
        (name "BAT+L/BAT+R" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
        (alternate "BAT+R" power_in line)
      )
      (pin power_in line (at 6.350 -29.210 90) (length 5.080)
        (name "BAT-" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "BSS84" (in_bom yes) (on_board yes)
    (property "Reference" "VT" (at 1.778 4.572 0)
      (effects (font (size 1.27 1.27)) (justify right bottom))
    )
    (property "Value" "BSS84" (at 1.778 -4.572 0)
      (effects (font (size 1.27 1.27)) (justify right top))
    )
    (property "Footprint" "qeda:SOT95P237X112-3N" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BSS84.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "transistor, MOSFET, p-channel, enhancement mode, GSD" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "BSS84_1_1"
      (circle (center 0.000 0.000) (radius 3.810)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -0.953 2.540)
          (xy -0.953 1.223)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.953 0.659)
          (xy -0.953 -0.659)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.953 -1.223)
          (xy -0.953 -2.540)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.953 -1.881)
          (xy 3.810 -1.881)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 3.810 -1.881)
          (xy 3.810 -2.540)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.953 1.881)
          (xy 3.810 1.881)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 3.810 1.881)
          (xy 3.810 2.540)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -3.810 -2.540)
          (xy -1.715 -2.540)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.715 2.540)
          (xy -1.715 -2.540)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.953 0.000)
          (xy 0.953 0.000)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.953 0.000)
          (xy 0.953 -1.881)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts (xy 0.000 0.381) (xy 0.953 0.000) (xy 0.000 -0.381))
        (stroke (width 0.305) (type default))
        (fill (type outline))
      )
      (polyline
        (pts
          (xy 2.191 1.881)
          (xy 2.191 0.412)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.191 -0.412)
          (xy 2.191 -1.881)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts (xy 1.715 0.412) (xy 2.667 0.412) (xy 2.191 -0.412) (xy 1.715 0.412))
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.715 -0.412)
          (xy 2.667 -0.412)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (pin input line (at -8.890 -2.540 0) (length 5.080)
        (name "G" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at 3.810 7.620 270) (length 5.080)
        (name "D" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at 3.810 -7.620 90) (length 5.080)
        (name "S" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "BSS138" (in_bom yes) (on_board yes)
    (property "Reference" "VT" (at 1.778 4.572 0)
      (effects (font (size 1.27 1.27)) (justify right bottom))
    )
    (property "Value" "BSS138" (at 1.778 -4.572 0)
      (effects (font (size 1.27 1.27)) (justify right top))
    )
    (property "Footprint" "qeda:SOT95P237X112-3N" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.onsemi.com/pdf/datasheet/bss138-d.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "transistor, MOSFET, n-channel, enhancement mode vertical DMOS, GSD" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "BSS138_1_1"
      (circle (center 0.000 0.000) (radius 3.810)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -0.953 2.540)
          (xy -0.953 1.223)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.953 0.659)
          (xy -0.953 -0.659)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.953 -1.223)
          (xy -0.953 -2.540)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.953 -1.881)
          (xy 3.810 -1.881)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 3.810 -1.881)
          (xy 3.810 -2.540)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.953 1.881)
          (xy 3.810 1.881)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 3.810 1.881)
          (xy 3.810 2.540)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -3.810 -2.540)
          (xy -1.715 -2.540)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -1.715 2.540)
          (xy -1.715 -2.540)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy -0.953 0.000)
          (xy 0.953 0.000)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.953 0.000)
          (xy 0.953 -1.881)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts (xy 0.000 0.381) (xy -0.953 0.000) (xy 0.000 -0.381))
        (stroke (width 0.305) (type default))
        (fill (type outline))
      )
      (polyline
        (pts
          (xy 2.191 1.881)
          (xy 2.191 0.412)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 2.191 -0.412)
          (xy 2.191 -1.881)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts (xy 1.715 -0.412) (xy 2.667 -0.412) (xy 2.191 0.412) (xy 1.715 -0.412))
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.715 0.412)
          (xy 2.667 0.412)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (pin input line (at -8.890 -2.540 0) (length 5.080)
        (name "G" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 3.810 7.620 270) (length 5.080)
        (name "D" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 3.810 -7.620 90) (length 5.080)
        (name "S" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "1206SFH" (pin_numbers hide) (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "F" (at 0.000 1.778 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "1206SFH" (at 0.000 -1.778 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "qeda:FUSC3215X117N" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "1206 (3216mm) High-Current-Rated Chip Fuse" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "Fuse" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "1206SFH_1_1"
      (rectangle (start -2.540 1.016) (end 2.540 -1.016)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy -2.540 0.000)
          (xy 2.540 0.000)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (pin passive line (at -3.810 0.000 0) (length 1.270)
        (name "L" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 3.810 0.000 180) (length 1.270)
        (name "R" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "XC6206" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 8.255 0.762 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "XC6206" (at 8.382 -9.652 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "qeda:SOT95P280X130-3N" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.torexsemi.com/file/xc6206/XC6206.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "positive voltage regulators" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "IC, regulator" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "XC6206_1_1"
      (rectangle (start 0.000 0.000) (end 16.510 -8.890)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (pin power_in line (at -5.080 -2.540 0) (length 5.080)
        (name "VIN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin unspecified line (at 21.590 -2.540 180) (length 5.080)
        (name "VOUT" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 7.620 -13.970 90) (length 5.080)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "SCHOTTKY" (pin_numbers hide) (pin_names hide) (in_bom yes) (on_board yes)
    (property "Reference" "D" (at 0.000 2.032 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "SCHOTTKY" (at 0.000 -2.032 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "qeda:SOD2513X110N" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "~" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "diode, schottky, generic" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SCHOTTKY_1_1"
      (polyline
        (pts (xy -1.016 1.270) (xy 1.016 0.000) (xy -1.016 -1.270) (xy -1.016 1.270))
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (polyline
        (pts
          (xy 1.016 1.270)
          (xy 1.016 -1.270)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.016 -1.270)
          (xy 0.508 -1.270)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 0.508 -1.270)
          (xy 0.508 -0.762)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.016 1.270)
          (xy 1.524 1.270)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (polyline
        (pts
          (xy 1.524 1.270)
          (xy 1.524 0.762)
        )
        (stroke (width 0.305) (type default))
        (fill (type none))
      )
      (pin passive line (at -2.540 0.000 0) (length 1.524)
        (name "A" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 2.540 0.000 180) (length 1.524)
        (name "C" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "STM32F103C" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at 0.000 0.762 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "STM32F103C" (at 23.622 -74.422 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "qeda:QFP50P900X900X160-48N" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.st.com/en/microcontrollers-microprocessors/stm32f030c8.html" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "ARM Cartex-M0 micro-controller" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_keywords" "IC, MCU, Micro-Controller, STM32, STM32F030" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "STM32F103C_1_1"
      (rectangle (start 0.000 0.000) (end 27.940 -73.660)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (pin input inverted (at -5.080 -2.540 0) (length 5.080)
        (name "NRST" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.080 -5.080 0) (length 5.080)
        (name "BOOT0" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -10.160 0) (length 5.080)
        (name "PA0" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -12.700 0) (length 5.080)
        (name "PA1" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -15.240 0) (length 5.080)
        (name "PA2" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -17.780 0) (length 5.080)
        (name "PA3" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -20.320 0) (length 5.080)
        (name "PA4" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -22.860 0) (length 5.080)
        (name "PA5" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -25.400 0) (length 5.080)
        (name "PA6" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -27.940 0) (length 5.080)
        (name "PA7" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -30.480 0) (length 5.080)
        (name "PA8" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -33.020 0) (length 5.080)
        (name "PA9" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -35.560 0) (length 5.080)
        (name "PA10" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -38.100 0) (length 5.080)
        (name "PA11" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -40.640 0) (length 5.080)
        (name "PA12" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -43.180 0) (length 5.080)
        (name "PA13-SWDIO" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -45.720 0) (length 5.080)
        (name "PA14-SWCLK" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -48.260 0) (length 5.080)
        (name "PA15" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -53.340 0) (length 5.080)
        (name "PC13" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -55.880 0) (length 5.080)
        (name "PC14-OSC32_IN" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -58.420 0) (length 5.080)
        (name "PC15-OSC32_OUT" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -63.500 0) (length 5.080)
        (name "PF0-OSC_IN" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -66.040 0) (length 5.080)
        (name "PF1-OSC_OUT" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -68.580 0) (length 5.080)
        (name "PF6-GBD" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.080 -71.120 0) (length 5.080)
        (name "PF7-VDD" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 33.020 -17.780 180) (length 5.080)
        (name "PB0" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 33.020 -20.320 180) (length 5.080)
        (name "PB1" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 33.020 -22.860 180) (length 5.080)
        (name "PB2" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 33.020 -25.400 180) (length 5.080)
        (name "PB3" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 33.020 -27.940 180) (length 5.080)
        (name "PB4" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 33.020 -30.480 180) (length 5.080)
        (name "PB5" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 33.020 -33.020 180) (length 5.080)
        (name "PB6" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 33.020 -35.560 180) (length 5.080)
        (name "PB7" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 33.020 -38.100 180) (length 5.080)
        (name "PB8" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 33.020 -40.640 180) (length 5.080)
        (name "PB9" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 33.020 -43.180 180) (length 5.080)
        (name "PB10" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 33.020 -45.720 180) (length 5.080)
        (name "PB11" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 33.020 -48.260 180) (length 5.080)
        (name "PB12" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 33.020 -50.800 180) (length 5.080)
        (name "PB13" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 33.020 -53.340 180) (length 5.080)
        (name "PB14" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 33.020 -55.880 180) (length 5.080)
        (name "PB15" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 16.510 5.080 270) (length 5.080)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 19.050 5.080 270) (length 5.080)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 21.590 5.080 270) (length 5.080)
        (name "VDD" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 24.130 5.080 270) (length 5.080)
        (name "VDDA" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.780 -78.740 90) (length 5.080)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 20.320 -78.740 90) (length 5.080)
        (name "VSS" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.860 -78.740 90) (length 5.080)
        (name "VSSA" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "TS-1187A" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 6.350 0.762 0)
      (effects (font (size 1.27 1.27)) (justify bottom))
    )
    (property "Value" "TS-1187A" (at 6.350 -8.382 0)
      (effects (font (size 1.27 1.27)) (justify top))
    )
    (property "Footprint" "qeda:MECHANICAL_TS-1187A" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.helloxkb.com/public/images/pdf/TS-1187A-X-X-X.pdf" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "ki_description" "dual tactical momentary switch, SMD 5.1*5.1*1.5mm" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TS-1187A_1_1"
      (rectangle (start 0.000 0.000) (end 12.700 -7.620)
        (stroke (width 0.305) (type default))
        (fill (type background))
      )
      (pin passive line (at -5.080 -2.540 0) (length 5.080)
        (name "A" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -5.080 -5.080 0) (length 5.080)
        (name "B" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 17.780 -2.540 180) (length 5.080)
        (name "C" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 17.780 -5.080 180) (length 5.080)
        (name "D" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
